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 The WORLD pallet in Europe
The most important in brief and facts
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WORLD PALLET AG

® Returnable / reusable pallet / exchange pallet
identical in construction with EPAL / EUR Pallets

* Worldwide application and exchangeable*
©6.000 kg lower load range —

with full-sureface stracking

e In the future accepted worldwide
by production in all continents

® 100 % quality warranty
for High rack-stackable

* according to IPPC / ISPM15 standard

www.world-pallet.com





WORLD pallets are manufactured with a licence from WORLD PALLET AG and the exclusive licence rights for the European market are held by Falkenhahn AG. Falkenhahn AG has been manufacturing Euro-pallets for more than 20 years. After 16 years under the EPAL licence, in 2008, Falkenhahn attained the exclusive licence rights for the production of the WORLD pallet in Europe.
Technical Specifications
· Dimension


800 x 1.200 x 144 mm
· Material


Wood
· Exchangeable pallets 
according DIN EN 13698-1

· Carrying capacity

1.200 to 2.200 kg depending on loading






6.000 kg with full-surface stracking
· Construction


identical with EPAL / EUR pallets
· Quality



100% warranty for High rack-stackable


Special Solutions on request
· ISPM 15 Treatment
The pallet can be delivered with ISPM 15 Standard
· Kiln dried
Moisture content below 20% - especially for the food and pharmaceutical industry
· Blocks
solid wood or compassed blocks available
· RFID

RFID pallet facilitates the automated identification of pallets and goods, thus an automatic inventory management.
Possible fields of application
The WORLD Pallet is employed in all industrial and commercial sectors as a 

returnable – reusable – exchangeable pallet
As a reusable and exchangeable pallet, the WORLD pallet is employed in the already existing fully automated production processes, for instance during loading and off-loading, in high bay warehouses and material handling technology. It is also employed as an export pallet in the market already. This militates in favor of its quality and high bearing load.
Advantages fields of application
· High rack-stackable
· All fields with high load capacity
· Worldwide application and exchangeable
· chemical and pharmaceutical sectors, automobile, steel and construction industry 
right to the packaging, synthetic material and foodstuff sectors.
The WORLD Pallet in the Euro-pallet format is being produced in a fully automated manufacturing process and on innovated plants and equipments. For a 100% quality control, each pallet, at the end of the manufacturing process, undergoes a full automated measurement of contours.

Further Information: 

WORLD PALLET AG, Felbaweg 10, FL – 9494 Schaan

mail: info@world-pallet.com;  web: www.world-pallet.com
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